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Creating a method based on standard parameter
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After switching on, the Titration Unit TitroLine alpha
shows the actual version number: in this case 94/47.







The first step after switched-on is filling. In the next step the actual unit must be confirmed or changed with <up / down>.



„Method 1“ can be started. For the first time it
must be created as described in the next steps.



Here it is possible to create methods. With <STD> it is
possible to create a method with standard parameter sets.


3 x
An overview is shown in the „List of the standard parameter“ (see above).











Example <<acid>> is selected.







The „acid“ examples show several selected examples.
It is shown the same type, not the titration reagent.







Other acids can be selected with the arrow keys
or with the input of the „number“.



In this example <<hydrochloric acid>> is selected.







In this example the parameters of the hydrochloric acid
are stored in „method 1“.







The selected titration now can run.











In the case of modifying the method, call up the „MODE“ menu and select <<MTH>>.







The method is parameterized; it is possible to adjust to the application. *)



Select <<y>> in the case of weight or sample volume.











The name of the method can be changed individually.







Define and select weight or sample volume. Possible other parameter see  *)







The modified method must be saved here.



Quit level of developing method to start the titration.







These keys allow the selection of other methods.



The titration can be started.



The calculation can be adjusted with <MODE> and <<CALC>>, the documentation with <<DOC>>.

*)
In the menu <INIT> you must switch on the menu point „editing standard parameters“ in <SYS> in the

case you want to change the predefined titration parameters. Then it is possible to change the parameters.
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ROLL�UP





ROLL�DOWN





	Mth�	1�<START>/<up/dwn>�	hydrochloric acid





ESC





		Mth�		1� method� test / store





ENTER





			Mth�			1�select weight�	wght.	vol.	none





ENTER





	Mth


	1�method name�	hydrochloric acid





ENTER





			Mth�			1�change method�	yes	no





			Mth�			1�change method�	yes	no





ENTER





	Mth


	1�MTH CALC DOC STD�LIST  PRN  MEAS





MODE





	Mth�	1�<START>/<up/dwn>�	hydrochloric acid





1





	STD�	10�--> work method no.�     store  <ENTER>





ENTER





ENTER





	STD�	10�next method   <<-/->>�	hydrochloric acid





ENTER





	STD�	10� Acid   Base   mV� pHstat        KF    ?





ENTER





�MTH CALC DOC STD�LIST  PRN  MEAS





�MTH CALC DOC STD�LIST  PRN  MEAS





		Mth�		1�<START>/<up/dwn>





MODE





50 ml


Unit OK? <ENTER>�10 20 50 <up/dwn>





ENTER
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